JEL PRODUCTS - PHOTOMETRIC FILES
================================
Linear
Issued 27 August 2026

This archive holds the photometric files for the JEL Products Linear range,
24 versions in EULUMDAT format (.ldt). DIALux and Relux read these
natively: drag the file into your project or import it as a luminaire.

FILE NAMES
<article number>_<product and version>_<power>_<optic>_<luminous flux>
Example: ORSS01-65K_Orca-SS-AC_800W_38deg_111300lm.ldt
The article number is the code to order by. It is stored inside every file
as well, so it stays with the file after downloading.

FOLDERS
One folder per version, with standard, SS and HT kept apart. Where the size
is what tells two versions apart, there is one more folder per length,
wattage or type.

LUMINOUS AREA
Equal to the luminaire size. This family has no non-emitting border.
The height of the luminous area is zero, because the lens is flat.

NEED AN IES FILE INSTEAD?
Ask us and we will send the IESNA LM-63 set for this range.

QUESTIONS
JEL Products - www.jelproducts.nl - info@jelproducts.nl - +31 (0)33 785 9809
